Slope of Control Column

in Neutral Elevator Position approx 10 degrees forward slope

Movement of Control Column approx 10 degrees forward for "down elevator"

approx 10 degrees backwards for "up elevator"
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